{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Расчёт"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Расчёт","index":0,"n_rows":4,"n_cols":18,"rows_kept":4,"cut":false,"hidden":false,"merged":[[0,0,0,9]],"flags":["formulas_cached_only"]}
["В меню Сервис-Параметры-Вычисления включите итерации.            ВВОДИТЬ ДАННЫЕ ТОЛЬКО В ЖЁЛТЫХ ЯЧЕЙКАХ !"]
[]
["Dвнутр      мм","  l,    м","G,     т/ч","v,     м/с","Re","kэкв ,     мм","l","R,  мм в. ст.  /м","hдл ,         мм в. ст.","доля м.с.,  %","hS ,       м в. ст.","hрасп нач ,     м в. ст.","hрасп кон ,     м в. ст.",null,"tпр,        oC","tобр,      oC","r, кг/м3","h, ПаЧс"]
[50,400,4.3,0.61,31950,0.5,0.0398,15.06,6024,10,6.626,30,23.37,0.0397,20,19,997.9,0.000952]