{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[{"$nulls":4},"ТОЧКА РОСЫ"]
[]
[null,"Исходные данные"]
[null,"Число Авогадро",null,"22,4л/гмоль"]
[null,"СН4+ 2О2=СО2+2Н2О"]
[null,"Вес 1 гмоля воды",null,"18г"]
["                   Точка росы без учета влажности воздуха поступающего на горение"]
[]
[]
[null,"Избыток воздуха ","Влажность кг/м3","Точка росы"]
[null,1,0.15277023356871267,63]
[null,1.2,0.12730852797392722,60]
[null,1.4,0.10912159540622333,56]
[null,1.6,0.09548139598044542,53]
[null,1.8,0.08487235198261815,50]
[null,2,0.07638511678435633,48]
[]
[null,"С влажностью воздуха подающегося на горение 10 г/м3(t=25, влажн=50%)"]
[]
[null,1,null,0.16477023356871268,"кг/м³",65,"ºС"]
[null,1.2,null,0.13730852797392723,"кг/м³",61,"ºС"]
[null,1.4,null,0.13730852797392723,"кг/м³",58,"ºС"]
[null,1.6,null,0.11769302397765193,"кг/м³",54,"ºС"]
[null,1.8,null,0.10298139598044542,"кг/м³",52,"ºС"]
[null,2,null,0.09153901864928482,"кг/м³",49.5,"ºС"]
[null,null,null," "]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}