{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":71,"n_cols":3,"rows_kept":71,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["NN","Наименование","Кол-во"]
[0,"Котел 50 кВт",1]
[1,"Радиатор панельный С11 500х400",3]
[2,"Радиатор панельный С11 500х800",2]
[3,"Радиатор панельный С11 500х1000",4]
[4,"Радиатор панельный С22 500х400",16]
[5,"Радиатор панельный С22 500х800",3]
[6,"Радиатор панельный С22 500х1000",4]
[7,"Радиатор панельный С22 500х1100",3]
[8,"Радиатор панельный С22 500х1200",1]
[9,"Радиатор панельный С22 600х2600",1]
[10,"Соединительная трубка 16-U",74]
[11,"Фитинг для соединительной  трубки  16-U",74]
[12,"Запорный вентиль",37]
[13,"Регулирующий вентиль",37]
[14,"Крестовина 20-16-16",2]
[15,"Крестовина 20-16-20",3]
[16,"Крестовина 25-20-20",2]
[17,"Тройник 16",38]
[18,"Тройник 20-16-16",4]
[19,"Тройник 20-16-20",2]
[20,"Тройник 20-25-20",4]
[21,"Тройник 25",2]
[22,"Тройник 25-16-25",2]
[23,"Муфта переходная 20х16",6]
[24,"Муфта комбинированная 25х3/4\" с вн.р.",6]
[25,"Направляющая дуга 25",12]
[26,"Угольник 25х90",12]
[27,"Угольник 25х3/4\"",2]
[28,"Труба   16 PEX",280]
[29,"Труба   20 PEX",80]
[30,"Труба   16 стабильная",150]
[31,"Труба   20 стабильная",150]
[32,"Труба   25 стабильная",50]
[33,"Гильза 16 PEX",110]
[34,"Гильза 20 PEX",50]
[35,"Гильза 16 стабильная",125]
[36,"Гильза 20 стабильная",5]
[37,"Гильза 25 стабильная",25]
[38,"Труба гофрированная из нерж.стали 3/4\" Dy20",2]
[39,"Труба гофрированная из нерж.стали 1 1/4\" Dy32",4]
[40,"Муфта комбин. DN 20х3/4\"",2]
[41,"Муфта комбин. DN 32х1 1/4\"",4]
[42,"Консоль для расшир. бака",1]
[43,"Расширительный бак 50 л",1]
[44,"Отсекатель для расшир. бака 3/4\"",1]
[45,"Предохран. клапан с манометром",1]
[46,"Кран шаровый 1 1/4\" вн./нар.",2]
[47,"Деаэратор 1 1/4\"",1]
[48,"Насос GRUNDFOS UPS-32 -80",1]
[49,"Коллектор 1 1/4\" на 4 выхода по 1/2\"",2]
[50,"Кран шар. с \"американкой\" 1/2\" вн./нар.",8]
[51,"Заглушка коллектора 1 1/4\"х1/2\"х1/2\"",2]
[52,"Заглушка 1/2\"",2]
[53,"Сливной кран 1/2\" (со штуцером)",3]
[54,"Труба дымохода 175мм - 1 м",1]
[55,"Отвод дымохода 175мм  - 45",2]
[56,"Футорка 3/4\"х1/2\"",4]
[57,"Фильтр \"сеточка\"",1]
[58,"Ниппель 1/2\" х 3/4\"",1]
[59,"Ниппель 1/2\"",1]
[60,"Ниппель 1 1/4\"",2]
[61,"Теплоизоляция \"Энергофлекс\" 18*6",150]
[62,"Теплоизоляция \"Энергофлекс\" 22*6",150]
[63,"Теплоизоляция \"Энергофлекс\" 28*6",50]
[64,"Теплоизоляция \"Энергофлекс\" 35*9",10]
[65,"Крепление для труб 16*2",200]
[66,"Крепление для труб 20*2",200]
[67,"Крепление для труб 26*2",50]
[68,"Дюбель 6*35",500]
[69,"Саморез 3,5*35",500]