{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["condensate"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"condensate","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
["Pr.","P&ID code","Description","Manufacturer","Type"]
[null,"0000.00.01","Condensate tank","Bi-N System","V= 1 м3 Drawing 144.001"]
[null,"0000.00.02","Level indicator","KSB Kuebler","KSR By-Pass Level Indicator with Level Sensing Element and Drog Magnet Indication"]
[null,"0000.00.03","Control console","-","-----"]
[null,"0000.00.04","FABA Long Life","ARI","12.046, flanged, PN16, DN65, GGG-40"]
[null,"0000.00.05","FABA Long Life","ARI","12.046, flanged, PN16, DN65, GGG-40"]
[null,"0000.00.06","FABA Long Life","ARI","12.046, flanged, PN16, DN65, GGG-40"]
[null,"0000.00.07","FABA Long Life","ARI","12.046, flanged, PN16, DN65, GGG-40"]
[null,"0000.00.08","Strainer","ARI","12.050, flanged, PN16, DN65, 1.4408"]
[null,"0000.00.09","Strainer","ARI","12.050, flanged, PN16, DN65, 1.4408"]
[null,"0000.00.10","Bimetal thermometer standard series","WIKA","R5242, 0-1200C, G1/2`"]
[null,"0000.00.11","Bimetal thermometer standard series","WIKA","R5242, 0-1200C, G1/2`"]
[null,"0000.00.12","Safety pressure gauge","WIKA","model 232.50, Ø100mm, 0/ 6 bar (G 1/2\" B, male, stainless steel), radial location of threaded entry design EN837-1, stainless steel casing 1.4571"]
[null,"0000.00.13","Safety pressure gauge","WIKA","model 232.50, Ø100mm, 0/ 6 bar (G 1/2\" B, male, stainless steel), radial location of threaded entry design EN837-1, stainless steel casing 1.4571"]
[null,"0000.00.14","Safety pressure gauge","WIKA","model 232.50, Ø100mm, 0/ 6 bar (G 1/2\" B, male, stainless steel), radial location of threaded entry design EN837-1, stainless steel casing 1.4571"]
[null,"0000.00.15","Safety pressure gauge","WIKA","model 232.50, Ø100mm, 0/ 6 bar (G 1/2\" B, male, stainless steel), radial location of threaded entry design EN837-1, stainless steel casing 1.4571"]
[null,"0000.00.16","Needle valve","WIKA","1/2'', PN400, S004.16.100, 4582142, DIN16270, LH/RH."]
[null,"0000.00.17","Needle valve","WIKA","1/2'', PN400, S004.16.100, 4582142, DIN16270, LH/RH."]
[null,"0000.00.18","Needle valve","WIKA","1/2'', PN400, S004.16.100, 4582142, DIN16270, LH/RH."]
[null,"0000.00.19","Needle valve","WIKA","1/2'', PN400, S004.16.100, 4582142, DIN16270, LH/RH."]
[null,"0000.00.20","Circulation pump","GRUNDFOS","DNP 32-125/132."]
[null,"0000.00.21","Circulation pump","GRUNDFOS","DNP 32-125/132"]
[null,"0000.00.22","Check valve","ARI","PN16, DN65, GGG-40"]
[null,"0000.00.23","Check valve","ARI","PN16, DN65, GGG-40"]
[null,"0000.00.24","Drainage ball valve for welding ","Naval","steel AISI 316L, welded connection, DN20, PN40."]
[null,"0000.00.25","Drainage ball valve for welding ","Naval","steel AISI 316L, welded connection, DN20, PN40."]
[null,"0000.00.26","Drainage ball valve for welding ","Naval","steel AISI 316L, welded connection, DN20, PN40."]
[null,"0000.00.27","Controls valve, 12 шт","ARI","STEVI, FIG. 12.470, DN25, PN16, Kvs4, pneumatic actuator DP32, flanged"]