{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":66,"n_cols":27,"rows_kept":66,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
{"$rows_empty":17}
[{"$nulls":8},"тг",null,null,"      тг",null,null,"        тг",{"$nulls":5},"       тг",null,null,"     тг",null,null,"        тг"]
[]
[]
[]
[]
[]
[{"$nulls":9},"              контур отопления кухни и спальни",{"$nulls":11},"    контур отопления зала и комнаты Богдана"]
{"$rows_empty":7}
[{"$nulls":4},"воздух"]
[{"$nulls":6},"  предохр"]
[{"$nulls":6},"  клапан"]
[]
[]
[{"$nulls":20},"  тг"]
[{"$nulls":22},"              тг"]
[{"$nulls":8},"цн","          цн",null,"    цн"]
[]
[{"$nulls":20},"                         контур отопления санузла и коридора"]
{"$rows_empty":13}
[{"$nulls":13},"  цн управл. Термодатчиком"]
[{"$nulls":5},"          подпитка"]
[]
[]
[{"$nulls":4},"слив сист."]
[]
[]
[]
[{"$nulls":8},"ввод холодной воды"]
[]
[{"$nulls":25},"цн"]
[{"$nulls":21},"      контур ГВС"]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}