{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":10,"n_cols":2,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,0,0,1]],"flags":["formulas_cached_only"]}
["Укрупненный расчет затрат тепла на отопление и вентиляцию"]
["Температура наружного воздуха, гр.С",-38]
["Температура внутреннего воздуха, гр.С",18]
["Поправочный коэффициент для отопительной характеристики",0.92]
["Отапливаемый объем здания, куб.м.",5000]
["Удельная тепловая характеристика на отопление qо",0.5]
["Удельная тепловая характеристика на вентиляцию qв",0]
["Расход тепла на отопление, кВт",128.8]
["Расход тепла на вентиляцию, кВт",0]
["Общий раскод тепла, кВт",128.8]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}