{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":9,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":18,"n_cols":8,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,1,2,7],[4,1,4,6],[5,1,5,6],[6,1,7,6],[6,7,7,7],[8,1,8,6],[9,1,9,6],[10,1,11,6],[10,7,11,7],[17,1,17,6],[12,1,14,6],[12,7,14,7],[15,1,15,6],[16,1,16,6]],"flags":["formulas_cached_only"]}
[]
[null,"Расчёт толщины тепловой изоляции для систем отопления ( по нормированной плотности теплового потока)"]
[]
[]
[null,"Температура среды внутри изолируемого оборудования tв, С",{"$nulls":5},65]
[null,"Температура окружающей среды tн, С",{"$nulls":5},20]
[null,"Коэффициент теплопроводности изоляционного слоя λиз, Вт/(м*С)",{"$nulls":5},0.06]
[]
[null,"Условный диаметр изолируемой трубы dу, м",{"$nulls":5},0.04]
[null,"Толщина стенки трубы бст, м",{"$nulls":5},0.0035]
[null,"Термическое сопротивление теплоотдаче на наружной поверхности изоляции Rн, м*С/Вт",{"$nulls":5},0.45]
[]
[null,"Нормативная плотность теплового потока через поверхность изоляции трубопроводов, расположенных в помещении qf, Вт/м",{"$nulls":5},26.5]
[]
[]
[null,"Величина lnВ",{"$nulls":5},0.4705275860150944]
[null,"Величина В",{"$nulls":5},-0.753900690400009]
[null,"Требуемая толщина теплоизоляции биз, м",{"$nulls":5},-0.04121666622440021]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}