{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Диаграмма1","ИТП-МГ4.05 \"Поток\""],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Диаграмма1","index":0,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ИТП-МГ4.05 \"Поток\"","index":1,"n_rows":17,"n_cols":8,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,"Время",null,null,"q1, Вт/кв.м.","q2, Вт/кв.м.","q3, Вт/кв.м."]
[null,null,"07:00:09",null,null,11.85,0,0]
[null,null,"07:30:09",null,null,16.1,0,0]
[null,null,"08:00:09",null,null,17.55,0,0]
[null,null,"08:30:09",null,null,17.6,0,0]
[null,null,"09:00:09",null,null,17.9,0,0]
[null,null,"09:30:57",null,null,18.61,0,0]
[null,null,"10:00:57",null,null,19.93,0,0]
[null,null,"10:30:57",null,null,21.72,0,0]
[null,null,"11:00:57",null,null,22.7,0,0]
[null,null,"11:30:57",null,null,22.91,0,0]
[null,null,"12:00:57",null,null,23.8,0,0]
[null,null,"12:30:57",null,null,24,0,0]
[null,null,"13:00:57",null,null,25,0,0]
[null,null,"13:30:58",null,null,26.3,0,0]
[null,null,"14:00:58",null,null,26.7,0,0]
[null,null,"14:30:58",null,null,27,0,0]