{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":0,"comments":3,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["(Отопление Водопровод Канализация  автор Копьев)"]
[]
["Расчет естественной циркуляции двухтрубной попутной нетупиковой системы отопления"]
[]
[]
["Водимые велечины"]
[]
["тепловая мощность системы",null,null,null,"Qc",27.085,"тыс. ккал/ч"]
["температура подачи",null,null,null,"tг=",95]
["температура обратки",null,null,null,"tо=",70]
["естествнное циркул.давление",null,null,null,"Ре.тр.=",6,"кгс/м2"]
["высота от котла до верхней трубы",null,null,null,"hг=",2.26,"м"]
["гор.расстояние от главн.стояка до расчетного",null,null,null,"l=",10,"м"]
["сумма гориз послед участков",null,null,null,"∑l=",68,"м"]
["поправка на изоляцию гл стояка",null,null,null,"b=",0.4]
["высота от котла до радиатора",null,null,null,"h1=",0.3,"м"]
["среднее увелечение объема массы воды",null,null,null,"β=",0.64]
[]
["Выходные велечины"]
[]
["Емкость расширительного бака ",null,null,null,"V=",54.17,"л"]
["Расчетное циркуляционное давление",null,null,null,"∆Рр=",15.883039999999998,"кгс/м2",155.65379199999998,"Па"]