{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["над 10-м эт."],"not_rendered":{"charts":0,"images":6,"macros":0,"external_links":1,"defined_names":0,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"над 10-м эт.","index":0,"n_rows":50,"n_cols":13,"rows_kept":50,"cut":false,"hidden":false,"merged":[[1,1,1,7],[2,1,2,7],[4,1,4,5],[5,1,5,5],[6,1,6,5],[10,5,10,7],[11,3,11,7],[12,3,12,7],[41,5,41,7],[42,1,44,5],[42,6,42,7],[43,6,43,7],[44,6,44,7],[45,1,45,5],[45,6,45,7],[46,1,46,5],[46,6,46,7],[49,1,49,7],[47,1,47,5],[47,6,47,7],[48,1,48,5],[48,6,48,7]],"flags":["formulas_cached_only"]}
[]
[null,"Определение ГСОП для г.Тюмени "]
[null,"в соответствии со СНиП 23-02-2003. \"Тепловая защита зданий\"",{"$nulls":7},"Конструкция  перекрытия (сеч. 19-19)"]
[{"$nulls":11},"d, м","l, Вт/(м °С) "]
[null,"Расчетная температура внутреннего воздуха (°С)",{"$nulls":4},"tв",21,null,"Цем. - песч. стяжка",null,0.08,0.76]
[null,"Средняя температура отопительного периода (°С)",{"$nulls":4},"tот.пер.",-7.2,null,"Керамзит",null,0.08,0.17]
[null,"Продолжительностьотопительного периода (сут.)",{"$nulls":4},"zот.пер.",225,null,"Плита монолитная",null,0.12,1.92]
[{"$nulls":9},"Утеплитель – П-125",null,0.16808215527917156,0.042]
[null,"ГСОП",{"$nulls":5},6345]
[]
[{"$nulls":5},"табл. 4, СНиП 23-02-2003"]
[null,null,null,"Приведенное сопротивление теплопередаче"]
[null,"Здания и","ГСОП"," ограждающих конструкций,  Rred, м2°С/Вт",{"$nulls":5},"Конструкция  перекрытия (сеч. 19-19)"]
[null,"помещения",null,"стен","покрытий и ","перекрытий","окон и","фонарей",null,null,null,"d, м","l, Вт/(м °С) "]
[{"$nulls":4},"перекрытий","чердачных,","балконных",null,null,"Цем. - песч. стяжка",null,0.08,0.76]
[{"$nulls":4},"над","над","дверей",null,null,"Керамзит",null,0.08,0.17]
[{"$nulls":4},"проездами","холодными",null,null,null,"Плита монолитная",null,0.12,1.92]
[{"$nulls":5},"подпольями",null,null,null,"Утеплитель – П-125",null,0.060761655279171566,0.042]
[{"$nulls":5},"и подвалами"]
[null,"Жилые",2000,2.1,3.2,2.8,0.3,0.3]
[null,null,4000,2.8,4.2,3.7,0.45,0.35]
[null,null,6000,3.5,5.2,4.6,0.6,0.4,null,"Конструкция  перекрытия над 6-м этажом"]
[null,null,8000,4.2,6.2,5.5,0.7,0.45,null,null,null,"d, м","l, Вт/(м °С) "]
[null,null,10000,4.9,7.2,6.4,0.75,0.5,null,"Цем. - песч. стяжка",null,0.02,0.76]
[null,null,12000,5.6,8.2,7.3,0.8,0.55,null,"Утеплитель – ППЖ-200 по ТУ 67-16-207-93",null,0.2177722750080069,0.05]
[null,null,null,3.6207499999999997,5.3725000000000005,4.75525,null,0.408625,null,"Керамзит",null,0.02,0.17]
[null,"Обществ.",2000,1.8,2.4,2,0.3,0.3,null,"Цем. - песч. стяжка",null,0.02,0.76]
[null,null,4000,2.4,3.2,2.7,0.4,0.35,null,"Ж/б плита",null,0.22,1.92]
[null,null,6000,3,4,3.4,0.5,0.4]
[null,null,8000,3.6,4.8,4.1,0.6,0.45]
[null,null,10000,4.2,5.6,4.8,0.7,0.5,null,"Конструкция  перекрытия над 6-м этажом"]
[null,null,12000,4.8,6.4,5.5,0.8,0.55,null,null,null,"d, м","l, Вт/(м °С) "]
[null,null,null,3.1034999999999995,4.138,3.5207499999999996,0.51725,0.408625,null,"Утеплитель – мин. плита марки Венти-баттс",null,0.1476141705544287,0.037]
[null,"Произв.",2000,1.4,2,1.4,0.25,0.2,null,"Керамзит",null,0.1,0.17]
[null,null,4000,1.8,2.5,1.8,0.3,0.25,null,"Монолитная ж/б плита",null,0.12,1.92]
[null,null,6000,2.2,3,2.2,0.35,0.3]
[null,null,8000,2.6,3.5,2.6,0.4,0.35]
[null,null,10000,3,4,3,0.45,0.4]
[null,null,12000,3.4,4.5,3.4,0.5,0.45]
[null,null,null,2.269,3.0862499999999997,2.269,0.358625,0.30862500000000004]
[]
[{"$nulls":5},"табл. 7, СНиП 23-02-2003"]
[null,"Внутренняя поверхность ограждающих конструкций ",{"$nulls":4},"Коэффициент "]
[{"$nulls":6},"теплоотдачи"]
[{"$nulls":6},"aв, Вт/(м2×°С)"]
[null,"1. Стен, полов, гладких потолков, потолков с выступающими ребрами при отношении высоты h ребер к расстоянию а между гранями соседних ребер h/aЈ3  ",{"$nulls":4},8.7]
[null,"2. Потолков с выступающими ребрами при отношении  h/a>3  ",{"$nulls":4},7.6]
[null,"3. Окон",{"$nulls":4},8]
[null,"3. Зенитных фонарей",{"$nulls":4},9.9]
[null,"П р и м е ч а н и е: Коэффициент теплоотдачи aв внутренней поверхности ограждающих конструкций животноводческих и птицеводческих зданий следует принимать в соответствии со СНиП 2.10.03-84."]