{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Лист2","Лист1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист2","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист1","index":1,"n_rows":26,"n_cols":12,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Расчет теплопотерь дома."]
["Дом 8 х 8 м, цокольный и 1 этаж. Цокольный этаж заглублен на 1 м. Высота цокольного - 2 м."]
["Высота 1-го этажа - 2,5 м. Количество окон - 4, из них 3 площадью 1,5 м2 и одно - 2,25 м2."]
["Две двери, каждая площадью по 2 м2."]
[{"$nulls":7},45]
["Разница температур","oС",45]
["Поправочн коэфф на вентиляцию",null,1.3]
["Параметр","ед.изм","Стены","Фундамент","Окна","Двери","Пол","Потолок"]
["Теплосопротивление","м2·oС/Вт",1.73,3.3,0.54,0.8,2.2,3.08]
["Площадь","м2",246.95,32,32.32,5.6,64,343]
["Разница температур","oС",45,20,45,45,20,45]
["Теплопотери в час","кВт",6.423554913294798,0.19393939393939394,2.6933333333333334,0.31499999999999995,0.5818181818181818,5.011363636363636,null,null,"Керамзит",0.12]
["Общие теплопотери в час для огр. констр.","кВт",15.219009458749344,{"$nulls":7},"Пенополистерол",0.035]
["С учетом вентиляции, в час","кВт",19.78471229637415,{"$nulls":7},"Штукатурка 15мм",0.87]
["Итого теплопотерь в сутки","кВт",474.83309511297955]
["в расчете на 1 м.кв. площади дома, в час","кВт",0.15456806481542304]
[]
[]
["Разница температур","oС",23]
["Поправочн коэфф на вентиляцию",null,1.3]
["Спальная комната"]
["Параметр","ед.изм","Стены","Фундамент","Окна","Двери","Пол","Потолок"]
["Теплосопротивление","м2·oС/Вт",3.3,3.3,0.55,1.14,2.2,4.2]
["Площадь","м2",101.25,32,6.75,4,10.6088,64]
["Разница температур","oС",45,20,45,45,20,45]
["Теплопотери в час","кВт",1.3806818181818183,0.19393939393939394,0.5522727272727272,0.15789473684210528,0.09644363636363636,0.6857142857142857]