{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":2,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,2,0,10],[2,0,2,1],[2,3,2,5],[6,3,6,5],[2,6,2,8]],"flags":["formulas_cached_only"]}
[null,null,"Расчёт и построение штуцера врезки D 45 х 3,5 в D 76 "]
[]
["Раб. таблица",null,null,"Исходные данные",null,null,"Расчётные данные"]
[null,60,null,"D; мм","d; мм","s; мм","R мм","r; мм","L разв.; мм "]
[0,61.22404494439136,null,76,57,3.5,38,25,179.0707812546182]
[11.191923828413637,64.36222399545022]
[22.383847656827275,67.82502509226606,null,"Точки координат графика",null,null,"Превыш."]
[33.575771485240914,69.38182395749163,null,"Точка","Х","У","Z"]
[44.76769531365455,67.82502509226606,null,0,0,60,0]
[55.959619142068185,64.36222399545022,null,1,11.191923828413637,61.22404494439136,1.224044944391359]
[67.15154297048183,61.22404494439136,null,2,22.383847656827275,64.36222399545022,4.362223995450222]
[78.34346679889546,60,null,3,33.575771485240914,67.82502509226606,7.82502509226606]
[89.5353906273091,61.22404494439136,null,4,44.76769531365455,69.38182395749163,9.381823957491633]
[100.72731445572273,64.36222399545022,null,5,55.959619142068185,67.82502509226606,7.82502509226606]
[111.91923828413637,67.82502509226606,null,6,67.15154297048183,64.36222399545022,4.362223995450222]
[123.11116211255,69.38182395749163,null,7,78.34346679889546,61.22404494439136,1.224044944391359]
[134.30308594096365,67.82502509226606,null,8,89.5353906273091,60,0]
[145.49500976937728,64.36222399545022,null,9,100.72731445572273,61.22404494439136,1.224044944391359]
[156.68693359779093,61.22404494439136,null,10,111.91923828413637,64.36222399545022,4.362223995450222]
[167.87885742620455,60,null,11,123.11116211255,67.82502509226606,7.82502509226606]
[179.0707812546182,null,null,12,134.30308594096365,69.38182395749163,9.381823957491633]
[null,null,null,13,145.49500976937728,67.82502509226606,7.82502509226606]
[null,null,null,14,156.68693359779093,64.36222399545022,4.362223995450222]
[null,null,null,15,167.87885742620455,61.22404494439136,1.224044944391359]
[null,null,null,16,179.0707812546182,60,0]

{"sheet":"Лист2","index":1,"n_rows":41,"n_cols":2,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Вылет стрелы, м","Высота подъёма крюка,   м"]
[]
[0]
[5.5,12]
[6,12]
[6.5,12]
[7,12]
[7.5,12]
[8,11]
[8.5,9.9]
[9,9.1]
[9.5,8.3]
[10,7.6]
[10.5,7]
[11,6.4]
[11.5,5.8]
[12,5.4]
[12.5,5]
[13,4.6]
[13.5,4.2]
[14,3.9]
[14.5,3.6]
[15,3.3]
[15.5,3]
[16,2.8]
[16.5,2.6]
[17,2.4]
[17.5,2.2]
[18,2]
[18.5,1.8]
[19,1.6]
[19.5,1.4]
[20,1.2]
[20.5,1]
[21,0.9]
[21.5,0.8]
[22,0.7]
[22.5,0.6]
[23,0.5]
[23.5,0.4]
[24]

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}