{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Теплотехнический"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Теплотехнический","index":0,"n_rows":12,"n_cols":19,"rows_kept":12,"cut":false,"hidden":false,"merged":[[3,17,4,17],[3,18,4,18],[6,0,11,0],[6,1,11,1],[6,13,8,13],[6,16,9,16],[6,17,9,17],[6,18,9,18],[3,16,4,16],[3,8,4,8],[3,9,4,9],[3,10,4,10],[11,2,11,14],[3,11,3,13],[3,14,4,14],[3,15,4,15],[1,1,1,17],[2,0,2,18],[3,0,4,0],[3,1,4,1],[3,2,3,5],[3,6,4,6],[3,7,4,7],[416,0,421,0],[410,0,415,0]],"flags":["formulas_cached_only"]}
[]
[]
["Ведомость расчёта теплопотерь и бытовых теплопоступлений"]
["Номер помещения и его назначение","Температура внутренненго воздуха tв,⁰c","Характеристики ограждения",null,null,null,"Рачетная температура наружног воздуха tн,⁰c","Расчетная разность температур tв-tн,⁰c","Коэффициент n","Коэффициент теплопередачи ограждения k, Вт/(м2*⁰c)","Основные теплопотери, Вт   Q₀=k*A*(tв-tн)*n","Дополнительные теплопотери",null,null,"Суммарные дополнительные теплопотери, ∑Qд ,  Вт","Теплопотери с учетом добавок Qоб=Qо+Qд","Расход теплоты на нагревание инфильтрующегося воздуха Qин, Вт","Бытовые тепловыделения Q д.бт, Вт","Полные теплопотери, ∑Qтп, Вт"]
[null,null,"Наименование","Ориентация","Размеры а*б;а*h, м","Площадь А, м2",{"$nulls":5},"С учетом ориентации, ℅","При наличии двух или более наружных стен, %","На открывание дверей Qднд, Вт"]
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19]
[1,20,"СТ",null,"20*5",100,0,20,1,357,714000,10,5,null,107100,821100]
[null,null,"СТ",null,"20*5",100,0,20,1,357,714000,10,5,null,107100,821100]
[null,null,"СТ",null,"20*5",100,0,20,1,357,714000,10,5,null,107100,821100]
[null,null,"СТ",null,"20*5",100,0,20,1,357,714000,10,5,null,107100,821100]
[null,null,"ПТ",null,"20*6",300,0,20,0.9,357,1927800,10,5,null,289170,2216970]
[{"$nulls":15},5501370,7207.200000000001,null,5508577.2]