{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":34,"n_cols":14,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Температура прямой -",null,null,95,"°С"]
[null,"Температура обратной -",null,null,70,"°С"]
[]
[null,"Температура в помещении -",null,null,20,"°С"]
[{"$nulls":10},"ОБОЗНАЧЕНИЕ","КОЛ-ВО СЕК.",null,"НОМ. ТЕПЛОВОЙ ПОТОК"]
[null,"Температурный напор -",null,null,{"$f":"((E2+E3)/2)-E5","v":62.5},"°С",{"$nulls":4},"РБС-500-3-555",3,null,{"$f":"$E$9*L7","v":495.53571428571422}]
[{"$nulls":10},"РБС-500-4-740",4,null,{"$f":"$E$9*L8","v":660.71428571428567}]
[null,"Ном. тепловой поток -",null,null,{"$f":"(E7*185)/70","v":165.17857142857142},"Вт","500мм",null,null,null,"РБС-500-5-925",5,null,825.89285714285711]
[{"$nulls":10},"РБС-500-6-1110",6,null,991.07142857142844]
[null,"Ном. тепловой поток -",null,null,{"$f":"(E7*121)/70","v":108.03571428571429},"Вт","300мм",null,null,null,"РБС-500-7-1295",7,null,1156.25]
[{"$nulls":10},"РБС-500-8-1480",8,null,1321.4285714285713]
[{"$nulls":10},"РБС-500-9-1665",9,null,1486.6071428571427]
[{"$nulls":10},"РБС-500-10-1850",10,null,1651.7857142857142]
[{"$nulls":10},"РБС-500-11-2035",11,null,1816.9642857142856]
[{"$nulls":10},"РБС-500-12-2220",12,null,1982.1428571428569]
[{"$nulls":10},"РБС-500-13-2405",13,null,2147.3214285714284]
[{"$nulls":10},"РБС-500-14-2590",14,null,2312.5]
[{"$nulls":10},"РБС-500-15-2775",15,null,2477.6785714285711]
[]
[]
[{"$nulls":10},"РБС-300-3-363",3,null,{"$f":"$E$11*L22","v":324.10714285714289}]
[{"$nulls":10},"РБС-300-4-484",4,null,{"$f":"$E$11*L23","v":432.14285714285717}]
[{"$nulls":10},"РБС-300-5-605",5,null,540.17857142857144]
[{"$nulls":10},"РБС-300-6-726",6,null,648.21428571428578]
[{"$nulls":10},"РБС-300-7-847",7,null,756.25]
[{"$nulls":10},"РБС-300-8-968",8,null,864.28571428571433]
[{"$nulls":10},"РБС-300-9-1089",9,null,972.32142857142867]
[{"$nulls":10},"РБС-300-10-1210",10,null,1080.3571428571429]
[{"$nulls":10},"РБС-300-11-1331",11,null,1188.3928571428571]
[{"$nulls":10},"РБС-300-12-1452",12,null,1296.4285714285716]
[{"$nulls":10},"РБС-300-13-1573",13,null,1404.4642857142858]
[{"$nulls":10},"РБС-300-14-1694",14,null,1512.5]
[{"$nulls":10},"РБС-300-15-1815",15,null,1620.5357142857144]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}