{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":23,"n_cols":23,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
{"$rows_empty":15}
[null,"Ширина светового проема, В, м",1.2]
[]
[]
[null,"Ширина вертикальных строительных  солнцезащитных плоскостей, l2 м",0.5]
[]
[null,"Расстояние от солнцезащитных плоскостей до горизонтального края светового проема, s, м",0.15,null,null,{"$f":"E21+10","v":10},20,30,40,50,{"$f":"J21+10","v":60},{"$f":"K21+10","v":70},80,90,100,110,120,130,140,150,160,170,180]
[]
[{"$nulls":5},{"$f":"1-($C$16^-1)*($C$19*ABS(TAN(RADIANS(F21)))-$C$21)","v":1.0515304247048063},0.97334573572241567,0.88443738783765591,0.7753751536761333,{"$f":"1-($C$16^-1)*($C$19*ABS(TAN(RADIANS(J21)))-$C$21)","v":0.62843600308574588},{"$f":"1-($C$16^-1)*($C$19*ABS(TAN(RADIANS(K21)))-$C$21)","v":0.40331216351296806},-1.9782258106092465E-2,-1.238034091507378,-6801896782341279,-1.2380340915073798,-1.9782258106092909E-2,0.40331216351296739,0.62843600308574588,0.77537515367613308,0.88443738783765591,0.97334573572241556,1.0515304247048063,1.125]