{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":11,"n_cols":4,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[null,"∆Т=(Т1+Т2)/2  - Т3",null,"185- теплоотдача1 секциии"]
[]
[null,"∆Т при 16гр.с",{"$f":"(90+70)/2-16","v":64},{"$f":"185*C7/70","v":169.14285714285714}]
[null,"∆Т при 25гр.с",{"$f":"(90+70)/2-25","v":55},{"$f":"185*C8/70","v":145.35714285714286}]
[null,"∆Т при 22гр.с",{"$f":"(90+70)/2-16","v":64},169.14285714285714]
[null,"∆Т при 20гр.с",{"$f":"(90+70)/2-20","v":60},158.57142857142858]
[null,"∆Т при 18гр.с",{"$f":"(90+70)/2-18","v":62},163.85714285714286]