{"text_format":"2","workbook":"xls","n_sheets":6,"sheets":["ТД Св-ва Воды","Теплопроводность","плотность","Вязкость","Прандтль","Теплоёмкость"],"not_rendered":{"charts":25,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ТД Св-ва Воды","index":0,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["Вода"]
[null,"t, оС","p, кг/м3","Cp, кДж/(кг*оС)","λ, Вт/(м*ºС)","ν*106, м2/с","Pr"]
[null,10,999.7,4.191,0.58,1.306,9.45]
[null,20,998.2,4.183,0.597,1.006,7.03]
[null,30,995.7,4.174,0.612,0.805,5.45]
[null,40,992.2,4.174,0.627,0.659,4.36]
[null,50,988.1,4.174,0.64,0.556,3.59]
[null,60,983.1,4.179,0.65,0.478,3.03]
[null,70,977.8,4.187,0.662,0.415,2.58]
[null,80,971.8,4.195,0.669,0.365,2.23]
[null,90,965.3,4.208,0.676,0.326,1.97]
[null,100,958.4,4.22,0.684,0.295,1.75]
[null,110,951,4.233,0.685,0.272,1.6]
[null,120,943.1,4.25,0.687,0.252,1.47]
[null,130,934.6,4.269,0.687,0.234,1.36]

{"sheet":"Теплопроводность","index":1,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["t, оС","λтабл, Вт/(м*ºС)","λлин, Вт/(м*ºС)","∆лин,%","λэкс, Вт/(м*ºС)","∆экс,%","λпол2, Вт/(м*ºС)","∆пол2,%","λпол3, Вт/(м*ºС)","∆пол3,%"]
[10,0.58,0.5851000000000001,0.8793103448276043,0.5855455277217703,0.9561254692707423,0.5798,0.03448275862068586,0.5792637363640001,0.12694200620687565]
[20,0.597,0.5961000000000001,0.15075376884420452,0.5961807773169302,0.13722322999493733,0.5977,0.11725293132328878,0.596469669194,0.08883263082076327]
[30,0.612,0.6071000000000001,0.8006535947712262,0.6070091946993865,0.8154910621917427,0.6142,0.35947712418300326,0.612308152024,0.05035163790850166]
[40,0.627,0.6181000000000001,1.4194577352471942,0.6180342883710991,1.429938058835872,0.6293,0.3668261562998355,0.626745968854,0.04051533429026759]
[50,0.64,0.6291000000000001,1.7031249999999858,0.6292596305588665,1.6781827251771164,0.643,0.4687500000000004,0.639749903684,0.039077549375005766]
[60,0.65,0.6401000000000001,1.523076923076909,0.6406888583717575,1.4324833274219286,0.6553,0.8153846153846109,0.651286740514,0.19796007907692578]
[70,0.662,0.6511,1.6465256797583112,0.6523256749795676,1.4613784018780085,0.6662,0.6344410876132902,0.661323263344,0.1022260809667655]
[80,0.669,0.6621,1.0313901345291505,0.6641738508126777,0.7213974868942274,0.6757,1.001494768310901,0.669826256174,0.12350615455904428]
[90,0.676,0.6731,0.42899408284023866,0.6762372247837068,0.035092423625266565,0.6838,1.1538461538461418,0.6767625030040001,0.11279630236687099]

{"sheet":"плотность","index":2,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["t, оС","pтабл, кг/м3","pлин, кг/м3","∆лин,%","pэкс, кг/м3","∆экс,%","pпол2, кг/м3","∆пол2,%","pпол3, кг/м3","∆пол3,%"]
[10,999.7,1002.328,0.26287886365909063,1002.1765690428697,0.24773122365406036,999.508,0.01920576172851928,999.553,0.01470441132340184]
[20,998.2,997.756,0.044480064115415115,997.1781925521622,0.10236500178700528,997.6360000000001,0.05650170306551438,998.026,0.01743137647766899]
[30,995.7,993.184,0.25268655217435737,992.2047455682048,0.351034893220375,995.0840000000001,0.061866023902780495,995.479,0.022195440393693245]
[40,992.2,988.612,0.3616206409998064,987.2561037545639,0.49827617873776675,991.8520000000001,0.03507357387623023,991.972,0.02297923805684998]
[50,988.1,984.04,0.41088958607428994,982.3321433949367,0.583732072165099,987.94,0.0161926930472592,987.565,0.05414431737678051]
[60,983.1,979.468,0.3694435967856842,977.4327413900575,0.5764681731199841,983.3480000000001,0.02522632489065683,982.318,0.07954429864714059]
[70,977.8,974.896,0.2969932501534052,972.557775254621,0.5361244370401884,978.076,0.028226631212933864,976.291,0.15432603804457976]
[80,971.8,970.324,0.15188310351924256,967.7071231142199,0.4211645282753669,972.124,0.03334019345545062,969.544,0.23214653220827042]
[90,965.3,965.752,0.04682482129907782,962.8806637022983,0.25063050841206336,965.4920000000001,0.019890189578381953,962.137,0.32767015435615987]

{"sheet":"Вязкость","index":3,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["t, оС","νтабл* 106, м2/с","νлин* 106, м2/с","∆лин,%","ν'экс* 106, м2/с","∆экс,%","ν'пол2* 106, м2/с","∆пол2,%","ν'пол3* 106, м2/с","∆пол3,%"]
[10,1.306,1.2176,6.768759571209803,1.214494890580761,7.006516800860562,1.3606,4.180704441041346,1.354156431741,3.6873224916538994]
[20,1.006,1.1006,9.403578528827039,1.0287333235087008,2.259773708618373,1.1176,11.09343936381709,1.055077892151,4.878518106461232]
[30,0.805,0.9836,22.186335403726705,0.8713846876631903,8.246545051327983,0.9146,13.614906832298125,0.823620318961,2.313083100745331]
[40,0.659,0.8666,31.50227617602428,0.7381031182154116,12.003508075176267,0.7516,14.051593323216997,0.650570322171,1.279162037784531]
[50,0.556,0.7496,34.82014388489208,0.6252074667278178,12.447386102125492,0.6285999999999998,13.057553956834491,0.5267145117809999,5.267174140107935]
[60,0.478,0.6325999999999999,32.34309623430961,0.5295796302788923,10.790717631567437,0.5456000000000001,14.142259414225963,0.44283949779099996,7.35575360020921]
[70,0.415,0.5156,24.24096385542168,0.44857843153115035,8.091188320759125,0.5025999999999999,21.10843373493975,0.38973189020099985,6.088701156385573]
[80,0.365,0.39859999999999995,9.205479452054785,0.3799666711670483,4.100457853985837,0.49960000000000004,36.876712328767134,0.35817829901100007,1.8689591750684722]
[90,0.326,0.2816000000000001,13.619631901840473,0.32184933792953024,1.273209224070481,0.5366000000000002,64.60122699386508,0.3389653342209997,3.9770963868097278]

{"sheet":"Прандтль","index":4,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["t, оС","Prтабл","Prлин","∆лин,%","Prэкс","∆экс,%","Prпол2","∆пол2,%","Prпол3","∆пол3,%"]
[10,9.45,8.7649,7.249735449735434,8.699625811235913,7.940467605969164,9.932,5.100529100529113,9.8924708856,4.6822315936508]
[20,7.03,7.863900000000001,11.862019914651503,7.208637894611119,2.541079581950479,7.9319999999999995,12.8307254623044,7.4733611396,6.306701843527731]
[30,5.45,6.962900000000001,27.759633027522955,5.973183378589599,9.599695019992646,6.212,13.98165137614678,5.625568153599999,3.22143401100915]
[40,4.36,6.0619000000000005,39.034403669724774,4.9494675964971355,13.51989900222787,4.772,9.449541284403667,4.269510327600001,2.0754512018348508]
[50,3.59,5.160900000000001,43.75766016713094,4.101201643429113,14.23960009551848,3.612,0.6128133704735443,3.325606061600002,7.3647336601670705]
[60,3.03,4.259900000000001,40.59075907590763,3.398315999072203,12.155643533736079,2.7319999999999993,9.834983498349851,2.714273755599999,10.420008066006629]
[70,2.58,3.3589,30.18992248062016,2.8158946166553482,9.143202195943728,2.1320000000000014,17.364341085271263,2.3559318095999995,8.684813581395371]
[80,2.23,2.4579000000000004,10.219730941704055,2.333291693377953,4.631914501253491,1.8119999999999994,18.744394618834107,2.170998623600001,2.6458016322869518]
[90,1.97,1.5569000000000006,20.96954314720809,1.933399813396818,1.8578774925473087,1.7719999999999985,10.050761421319873,2.0798925976000024,5.578304446700634]

{"sheet":"Теплоёмкость","index":5,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["t, оС","Cpтабл, кДж/(кг*оС)","Cpлин,, кДж/(кг*оС)","∆лин,%","Cpэкс,, кДж/(кг*оС)","∆экс,%","Cpпол2,, кДж/(кг*оС)","∆пол2,%","Cpпол3,, кДж/(кг*оС)","∆пол3,%"]
[10,4.191,4.1815,0.22667621092818097,4.181425973971413,0.2284425203671447,4.194100000000001,0.07396802672395059,4.1937617581,0.06589735385349851]
[20,4.183,4.1845,0.03585943103036235,4.184353996841637,0.03236903757199926,4.186100000000001,0.07410949079609776,4.1825223291,0.011419337795831127]
[30,4.174,4.1875,0.3234307618591189,4.1872840700454015,0.3182575478054889,4.1821,0.19405845711547132,4.175754560100001,0.04203545999042144]
[40,4.174,4.190499999999999,0.3953042644944621,4.190216195018445,0.3885049117979146,4.1821,0.19405845711547132,4.1730636511000005,0.022432891710585243]
[50,4.174,4.193499999999999,0.46717776712982656,4.1931503731975095,0.45880146615977757,4.186100000000001,0.28988979396263104,4.174054802100001,0.001312939626262464]
[60,4.179,4.1964999999999995,0.4187604690117057,4.196086606020339,0.4088682943368924,4.194100000000001,0.3613304618329824,4.1783332131,0.015955656855709613]
[70,4.187,4.1995,0.29854310962501285,4.1990248949256905,0.28719596192238483,4.2061,0.4561738715070431,4.185504084100001,0.035727630761873526]
[80,4.195,4.2025,0.17878426698449096,4.2019652413533235,0.166036742629874,4.2221,0.646007151370677,4.195172615100001,0.0041147818832021075]
[90,4.208,4.2055,0.059410646387841985,4.204907646744009,0.07348748231918299,4.2421,0.8103612167300279,4.2069440061000005,0.02509491207223534]