{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[[19,1,19,5],[20,1,20,5],[13,1,13,5],[14,1,14,5],[15,1,15,5],[16,1,16,5],[17,1,17,5],[18,1,18,5]]}
[null,"Пятно застройки: квадрат 16х16"]
[]
["Зона","S","R","R*S","Tint","Text","Nдней","Q"]
["I",128,2.1,{"$f":"B4*C4","v":268.8},20,-2.2000000000000002,205,{"$f":"(E4-F4)/C4*G4*24*B4/1000","v":6657.4628571428566}]
["II",80,4.3,{"$f":"B5*C5","v":344},20,-2.2000000000000002,205,{"$f":"(E5-F5)/C5*G5*24*B5/1000","v":2032.0744186046516}]
["III",48,8.6,412.79999999999995,20,-2.2000000000000002,205,609.62232558139556]
["IV",16,14.2,227.2,20,-2.2000000000000002,205,123.06929577464791]
["Сумма",{"$f":"SUM(B4:B7)","v":272},null,{"$f":"SUM(D4:D7)","v":1252.8},20,-2.2000000000000002,205,{"$f":"SUM(H4:H7)","v":9422.2288971035523}]
[]
["Среднее",{"$f":"B8","v":272},{"$f":"D8/B8","v":4.6058823529411761},null,20,-2.2000000000000002,205,{"$f":"(E10-F10)/C10*G10*24*B10/1000","v":6450.2142528735621}]
[]
[]
[]
["Параметр","Расшифровка"]
["S","Площадь сегмента (или общая)"]
["R","Сопротивление теплопередаче"]
["R*S","Площадь х Сопротивление теплопередаче"]
["Tint","Температура в помещении"]
["Text","Средняя температура отопительного сезона"]
["Nдней","Продолжительность отопительного сезона"]
["Q","Тепловые потери за отопительный сезон"]