{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["РБ"],"not_rendered":{"charts":2,"images":0,"macros":0,"external_links":3,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"РБ","index":0,"n_rows":487,"n_cols":14,"rows_kept":487,"cut":false,"hidden":false,"merged":[[4,0,4,13],[5,0,5,13],[7,1,7,5],[8,1,8,5],[10,8,10,12],[28,7,29,7],[32,2,32,5],[33,2,33,5],[34,2,34,5],[41,6,41,7],[42,6,42,7],[48,2,49,7],[48,9,49,9],[55,5,56,5],[55,7,56,7],[66,2,67,9],[66,11,67,11],[104,1,104,5],[104,6,104,7],[104,8,104,9],[104,10,104,11],[105,1,105,11],[106,1,106,5],[106,6,106,7],[106,8,106,9],[106,10,106,11],[107,1,107,5],[107,6,107,7],[107,8,107,9],[107,10,107,11],[108,1,108,5],[108,6,108,7],[108,8,108,9],[108,10,108,11],[109,1,109,5],[109,6,109,7],[109,8,109,9],[109,10,109,11],[110,1,110,5],[110,6,110,7],[110,8,110,9],[110,10,110,11],[111,1,111,5],[111,6,111,7],[111,8,111,9],[111,10,111,11],[112,1,112,5],[112,6,112,7],[112,8,112,9],[112,10,112,11],[113,1,113,5],[113,6,113,7],[113,8,113,9],[113,10,113,11],[114,1,114,5],[114,6,114,7],[114,8,114,9],[114,10,114,11],[115,1,115,5],[115,6,115,7],[115,8,115,9],[115,10,115,11],[116,1,116,5],[116,6,116,7],[116,8,116,9],[116,10,116,11],[117,1,117,11],[118,1,118,5],[118,6,118,7],[118,8,118,9],[118,10,118,11],[119,1,119,5],[119,6,119,7],[119,8,119,9],[119,10,119,11],[120,1,120,5],[120,6,120,7],[120,8,120,9],[120,10,120,11],[121,1,121,5],[121,6,121,7],[121,8,121,9],[121,10,121,11],[122,1,122,5],[122,6,122,7],[122,8,122,9],[122,10,122,11],[123,1,123,5],[123,6,123,7],[123,8,123,9],[123,10,123,11],[124,1,124,5],[124,6,124,7],[124,8,124,9],[124,10,124,11],[125,1,125,11],[126,1,126,5],[126,6,126,7],[126,8,126,9],[126,10,126,11],[127,1,127,5],[127,6,127,7],[127,8,127,9],[127,10,127,11],[128,1,128,5],[128,6,128,7],[128,8,128,9],[128,10,128,11],[129,1,129,5],[129,6,129,7],[129,8,129,9],[129,10,129,11],[130,1,130,5],[130,6,130,7],[130,8,130,9],[130,10,130,11],[131,1,131,5],[131,6,131,7],[131,8,131,9],[131,10,131,11],[132,1,132,5],[132,6,132,7],[132,8,132,9],[132,10,132,11],[133,1,133,5],[133,6,133,7],[133,8,133,9],[133,10,133,11],[134,1,134,5],[134,6,134,7],[134,8,134,9],[134,10,134,11],[135,1,135,11],[136,1,136,5],[136,6,136,7],[136,8,136,9],[136,10,136,11],[137,1,137,5],[137,6,137,7],[137,8,137,9],[137,10,137,11],[138,1,138,5],[138,6,138,7],[138,8,138,9],[138,10,138,11],[139,1,139,5],[139,6,139,7],[139,8,139,9],[139,10,139,11],[140,1,140,5],[140,6,140,7],[140,8,140,9],[140,10,140,11],[141,6,141,9],[141,10,141,11],[143,4,143,10],[145,4,145,5],[145,6,145,7],[145,9,145,10],[146,4,165,5],[146,6,146,7],[146,9,146,10],[147,6,147,7],[147,9,147,10],[148,6,148,7],[148,9,148,10],[149,6,149,7],[149,9,149,10],[150,6,150,7],[150,9,150,10],[151,6,151,7],[151,9,151,10],[152,6,152,7],[152,9,152,10],[153,6,153,7],[153,9,153,10],[154,6,154,7],[154,9,154,10],[155,6,155,7],[155,9,155,10],[156,6,156,7],[156,9,156,10],[157,6,157,7],[157,9,157,10],[158,6,158,7],[158,9,158,10],[159,6,159,7],[159,9,159,10],[160,6,160,7],[160,9,160,10],[161,6,161,7],[161,9,161,10],[162,6,162,7],[162,9,162,10],[163,6,163,7],[163,9,163,10],[164,6,164,7],[164,9,164,10],[165,6,165,7],[165,9,165,10],[166,4,185,5],[166,6,166,7],[166,9,166,10],[167,6,167,7],[167,9,167,10],[168,6,168,7],[168,9,168,10],[169,6,169,7],[169,9,169,10],[170,6,170,7],[170,9,170,10],[171,6,171,7],[171,9,171,10],[172,6,172,7],[172,9,172,10],[173,6,173,7],[173,9,173,10],[174,6,174,7],[174,9,174,10],[175,6,175,7],[175,9,175,10],[176,6,176,7],[176,9,176,10],[177,6,177,7],[177,9,177,10],[178,6,178,7],[178,9,178,10],[179,6,179,7],[179,9,179,10],[180,6,180,7],[180,9,180,10],[181,6,181,7],[181,9,181,10],[182,6,182,7],[182,9,182,10],[183,6,183,7],[183,9,183,10],[184,6,184,7],[184,9,184,10],[185,6,185,7],[185,9,185,10],[186,4,186,8],[186,9,186,10],[189,4,189,10],[191,4,191,5],[191,6,191,7],[191,9,191,10],[192,4,211,5],[192,6,192,7],[192,9,192,10],[193,6,193,7],[193,9,193,10],[194,6,194,7],[194,9,194,10],[195,6,195,7],[195,9,195,10],[196,6,196,7],[196,9,196,10],[197,6,197,7],[197,9,197,10],[198,6,198,7],[198,9,198,10],[199,6,199,7],[199,9,199,10],[200,6,200,7],[200,9,200,10],[201,6,201,7],[201,9,201,10],[202,6,202,7],[202,9,202,10],[203,6,203,7],[203,9,203,10],[204,6,204,7],[204,9,204,10],[205,6,205,7],[205,9,205,10],[206,6,206,7],[206,9,206,10],[207,6,207,7],[207,9,207,10],[208,6,208,7],[208,9,208,10],[209,6,209,7],[209,9,209,10],[210,6,210,7],[210,9,210,10],[211,6,211,7],[211,9,211,10],[212,4,231,5],[212,6,212,7],[212,9,212,10],[213,6,213,7],[213,9,213,10],[214,6,214,7],[214,9,214,10],[215,6,215,7],[215,9,215,10],[216,6,216,7],[216,9,216,10],[217,6,217,7],[217,9,217,10],[218,6,218,7],[218,9,218,10],[219,6,219,7],[219,9,219,10],[220,6,220,7],[220,9,220,10],[221,6,221,7],[221,9,221,10],[222,6,222,7],[222,9,222,10],[223,6,223,7],[223,9,223,10],[224,6,224,7],[224,9,224,10],[225,6,225,7],[225,9,225,10],[226,6,226,7],[226,9,226,10],[227,6,227,7],[227,9,227,10],[228,6,228,7],[228,9,228,10],[229,6,229,7],[229,9,229,10],[230,6,230,7],[230,9,230,10],[231,6,231,7],[231,9,231,10],[232,4,232,8],[232,9,232,10],[235,4,235,10],[237,4,237,5],[237,6,237,7],[237,9,237,10],[238,4,257,5],[238,6,238,7],[238,9,238,10],[239,6,239,7],[239,9,239,10],[240,6,240,7],[240,9,240,10],[241,6,241,7],[241,9,241,10],[242,6,242,7],[242,9,242,10],[243,6,243,7],[243,9,243,10],[244,6,244,7],[244,9,244,10],[245,6,245,7],[245,9,245,10],[246,6,246,7],[246,9,246,10],[247,6,247,7],[247,9,247,10],[248,6,248,7],[248,9,248,10],[249,6,249,7],[249,9,249,10],[250,6,250,7],[250,9,250,10],[251,6,251,7],[251,9,251,10],[252,6,252,7],[252,9,252,10],[253,6,253,7],[253,9,253,10],[254,6,254,7],[254,9,254,10],[255,6,255,7],[255,9,255,10],[256,6,256,7],[256,9,256,10],[257,6,257,7],[257,9,257,10],[258,4,277,5],[258,6,258,7],[258,9,258,10],[259,6,259,7],[259,9,259,10],[260,6,260,7],[260,9,260,10],[261,6,261,7],[261,9,261,10],[262,6,262,7],[262,9,262,10],[263,6,263,7],[263,9,263,10],[264,6,264,7],[264,9,264,10],[265,6,265,7],[265,9,265,10],[266,6,266,7],[266,9,266,10],[267,6,267,7],[267,9,267,10],[268,6,268,7],[268,9,268,10],[269,6,269,7],[269,9,269,10],[270,6,270,7],[270,9,270,10],[271,6,271,7],[271,9,271,10],[272,6,272,7],[272,9,272,10],[273,6,273,7],[273,9,273,10],[274,6,274,7],[274,9,274,10],[275,6,275,7],[275,9,275,10],[276,6,276,7],[276,9,276,10],[277,6,277,7],[277,9,277,10],[280,9,280,10],[281,6,281,7],[281,9,281,10],[282,6,282,7],[282,9,282,10],[283,6,283,7],[283,9,283,10],[284,6,284,7],[284,9,284,10],[285,6,285,7],[285,9,285,10],[286,6,286,7],[286,9,286,10],[287,6,287,7],[287,9,287,10],[288,6,288,7],[288,9,288,10],[289,6,289,7],[289,9,289,10],[290,6,290,7],[290,9,290,10],[291,6,291,7],[291,9,291,10],[292,6,292,7],[292,9,292,10],[293,6,293,7],[293,9,293,10],[294,6,294,7],[294,9,294,10],[295,6,295,7],[295,9,295,10],[296,6,296,7],[296,9,296,10],[297,6,297,7],[297,9,297,10],[298,4,298,8],[298,9,298,10],[278,4,297,5],[278,6,278,7],[278,9,278,10],[279,6,279,7],[279,9,279,10],[280,6,280,7],[301,4,301,10],[303,4,303,5],[303,9,303,10],[304,4,335,5],[304,6,317,6],[304,9,304,10],[305,9,305,10],[306,9,306,10],[307,9,307,10],[308,9,308,10],[309,9,309,10],[310,9,310,10],[311,9,311,10],[312,9,312,10],[313,9,313,10],[314,9,314,10],[315,9,315,10],[316,9,316,10],[317,9,317,10],[318,6,335,6],[318,9,318,10],[319,9,319,10],[320,9,320,10],[321,9,321,10],[322,9,322,10],[323,9,323,10],[324,9,324,10],[325,9,325,10],[326,9,326,10],[327,9,327,10],[328,9,328,10],[329,9,329,10],[330,9,330,10],[331,9,331,10],[332,9,332,10],[333,9,333,10],[334,9,334,10],[335,9,335,10],[336,4,367,5],[336,6,349,6],[336,9,336,10],[337,9,337,10],[338,9,338,10],[339,9,339,10],[340,9,340,10],[341,9,341,10],[342,9,342,10],[343,9,343,10],[344,9,344,10],[345,9,345,10],[346,9,346,10],[347,9,347,10],[348,9,348,10],[349,9,349,10],[350,6,367,6],[350,9,350,10],[351,9,351,10],[352,9,352,10],[353,9,353,10],[354,9,354,10],[355,9,355,10],[356,9,356,10],[357,9,357,10],[358,9,358,10],[359,9,359,10],[360,9,360,10],[361,9,361,10],[362,9,362,10],[363,9,363,10],[364,9,364,10],[365,9,365,10],[366,9,366,10],[367,9,367,10],[368,4,399,5],[368,6,381,6],[368,9,368,10],[369,9,369,10],[370,9,370,10],[371,9,371,10],[372,9,372,10],[373,9,373,10],[374,9,374,10],[375,9,375,10],[376,9,376,10],[377,9,377,10],[378,9,378,10],[379,9,379,10],[380,9,380,10],[381,9,381,10],[382,6,399,6],[382,9,382,10],[383,9,383,10],[384,9,384,10],[385,9,385,10],[386,9,386,10],[387,9,387,10],[388,9,388,10],[389,9,389,10],[390,9,390,10],[391,9,391,10],[392,9,392,10],[393,9,393,10],[394,9,394,10],[395,9,395,10],[396,9,396,10],[397,9,397,10],[398,9,398,10],[399,9,399,10],[400,4,400,8],[400,9,400,10],[404,4,404,5],[404,7,404,8],[404,9,404,10],[405,4,405,5],[405,7,405,8],[405,9,405,10],[406,4,406,5],[406,7,406,8],[406,9,406,10],[407,4,407,5],[407,7,407,8],[407,9,407,10],[408,4,408,5],[408,7,408,8],[408,9,408,10],[409,4,409,5],[409,7,409,8],[409,9,409,10],[410,4,410,5],[410,7,410,8],[410,9,410,10],[411,4,411,5],[411,7,411,8],[411,9,411,10],[412,4,412,5],[412,7,412,8],[412,9,412,10],[413,4,413,5],[413,7,413,8],[413,9,413,10],[414,4,414,5],[414,7,414,8],[414,9,414,10],[415,4,415,5],[415,7,415,8],[415,9,415,10],[416,4,416,5],[416,7,416,8],[416,9,416,10],[417,4,417,5],[417,7,417,8],[417,9,417,10],[418,4,418,5],[418,7,418,8],[418,9,418,10],[419,4,419,5],[419,7,419,8],[419,9,419,10],[420,4,420,5],[420,7,420,8],[420,9,420,10],[421,4,421,5],[421,7,421,8],[421,9,421,10],[422,4,422,5],[422,7,422,8],[422,9,422,10],[423,4,423,5],[423,7,423,8],[423,9,423,10],[424,4,424,5],[424,7,424,8],[424,9,424,10],[425,4,425,5],[425,7,425,8],[425,9,425,10],[426,4,426,5],[426,7,426,8],[426,9,426,10],[427,4,427,5],[427,7,427,8],[427,9,427,10],[428,4,428,5],[428,7,428,8],[428,9,428,10],[429,4,429,5],[429,7,429,8],[429,9,429,10],[430,4,430,5],[430,7,430,8],[430,9,430,10],[431,4,431,5],[431,7,431,8],[431,9,431,10],[432,4,432,5],[432,7,432,8],[432,9,432,10],[433,4,433,5],[433,7,433,8],[433,9,433,10],[434,4,434,5],[434,7,434,8],[434,9,434,10],[435,4,435,5],[435,7,435,8],[435,9,435,10],[436,4,436,5],[436,7,436,8],[436,9,436,10],[437,4,437,5],[437,7,437,8],[437,9,437,10],[438,4,438,5],[438,7,438,8],[438,9,438,10],[439,4,439,5],[439,7,439,8],[439,9,439,10],[440,4,440,5],[440,7,440,8],[440,9,440,10],[441,4,441,5],[441,7,441,8],[441,9,441,10],[442,4,442,5],[442,7,442,8],[442,9,442,10],[443,4,443,5],[443,7,443,8],[443,9,443,10],[444,4,444,5],[444,7,444,8],[444,9,444,10],[445,4,445,5],[445,7,445,8],[445,9,445,10],[446,4,446,5],[446,7,446,8],[446,9,446,10],[447,4,447,5],[447,7,447,8],[447,9,447,10],[448,4,448,5],[448,7,448,8],[448,9,448,10],[449,4,449,5],[449,7,449,8],[449,9,449,10],[450,4,450,5],[450,7,450,8],[450,9,450,10],[451,4,451,5],[451,7,451,8],[451,9,451,10],[452,4,452,5],[452,7,452,8],[452,9,452,10],[453,4,453,5],[453,7,453,8],[453,9,453,10],[454,4,454,5],[454,7,454,8],[454,9,454,10],[455,4,455,5],[455,7,455,8],[455,9,455,10],[456,4,456,5],[456,7,456,8],[456,9,456,10],[457,4,457,5],[457,7,457,8],[457,9,457,10],[458,4,458,5],[458,7,458,8],[458,9,458,10],[459,4,459,5],[459,7,459,8],[459,9,459,10],[460,4,460,5],[460,7,460,8],[460,9,460,10],[461,4,461,5],[461,7,461,8],[461,9,461,10],[462,4,462,5],[462,7,462,8],[462,9,462,10],[463,4,463,5],[463,7,463,8],[463,9,463,10],[464,4,464,8],[464,9,464,10],[467,3,467,5],[467,6,467,7],[467,8,467,9],[467,10,467,11],[468,3,468,5],[468,6,468,7],[468,8,468,9],[468,10,468,11],[469,3,469,5],[469,6,469,7],[469,8,469,9],[469,10,469,11],[470,3,470,5],[470,6,470,7],[470,8,470,9],[470,10,470,11],[471,3,471,5],[471,6,471,7],[471,8,471,9],[471,10,471,11],[472,3,472,5],[472,6,472,7],[472,8,472,9],[472,10,472,11],[473,3,473,5],[473,6,473,7],[473,8,473,9],[473,10,473,11],[474,3,474,5],[474,6,474,7],[474,8,474,9],[474,10,474,11],[475,3,475,5],[475,6,475,7],[475,8,475,9],[475,10,475,11],[476,3,476,5],[476,6,476,7],[476,8,476,9],[476,10,476,11],[477,3,477,5],[477,6,477,7],[477,8,477,9],[477,10,477,11],[478,3,478,5],[478,6,478,7],[478,8,478,9],[478,10,478,11],[479,3,479,5],[479,6,479,7],[479,8,479,9],[479,10,479,11],[480,3,480,5],[480,6,480,7],[480,8,480,9],[480,10,480,11],[481,3,481,5],[481,6,481,7],[481,8,481,9],[481,10,481,11],[482,3,482,5],[482,6,482,7],[482,8,482,9],[482,10,482,11],[483,3,483,9],[483,10,483,11],[486,3,486,9],[486,10,486,11]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
["      Расчет объёма расширительного сосуда"]
["   отопительной системы"]
[]
[null,"Таблица 1:   Зависимость коэффициента"]
[null," расширения  n в % от температуры жидкости"]
[null,null,"Вода","50% а.фр.","DIX 30","DIX 65"]
[null,"Т,оС","nв, %","n50%а/ф, %","nD30, %","nD65, %",null,null,"Исходные данные"]
[null,10,0.004,0.599,0.53,0.604]
[null,20,0.18,1.206,1.06,1.208,{"$nulls":5},"Температура воздуха в помещении на "]
[null,30,0.44,1.79,1.59,1.812,{"$nulls":5},"момент заполнения системы отопления, Тнач= ",10,",оС"]
[null,40,0.79,2.381,2.12,2.416]
[null,50,1.21,3.089,2.65,3.02,{"$nulls":5},"Температура теплоносителя на выходе из котла, Т1=",90,",оС"]
[null,60,1.71,3.808,3.18,3.624]
[null,70,2.28,4.577,3.71,4.228,{"$nulls":5},"Мощность отопительной установки, Q=",null,",кВт"]
[null,80,2.9,5.359,4.24,4.832]
[null,90,3.59,6.183,4.77,5.436,{"$nulls":5},"Статическая высота, hst=",3.3,",м"]
[null,100,4.35,7.021,5.3,6.04,{"$nulls":5},"(от точки установки РБ до верхней точки системы отопления)"]
[null,110,5.15,7.904,5.83,6.644,{"$nulls":5},"Давление настройки предохранительного клапана pSV=",3,", бар"]
[null,120,6.03,8.784,6.36,7.248]
[{"$nulls":11},"Высота расположения предохранительного клапана, hSV=",1.5,",м"]
[{"$nulls":11},"(от точки установки РБ до точки установки предохранительного клапана)"]
[]
[]
[{"$nulls":6},"Таблица 2:  Коэффициент объёмного расширения теплоносителя, n"]
[{"$nulls":5},"Т1","Тнач","n=n1-n2"]
[{"$nulls":5},"n1","n0"]
[{"$nulls":5},2.9,0.004,2.896]
[{"$nulls":6},"Таблица 3  Средний удельный объём теплоносителя в системе отопления при температуре на выходе из котла 90оС"]
[null,null,"Тип отопительных приборов",null,null,null,"Конвекто-ры","Вентиля-ционные установ-ки","Отопите-льные батареи","Радиато-ры","Трубопроводы","Отопле-ние пола"]
[null,null,"Доля мощности в системе отопления,m"]
[null,null,"Удельный объём системы v, л/кВт",null,null,null,5.1,6.9,9.4,12,17.2,19.8]
[]
[{"$nulls":6},"Таблица 3(справочная): Поправочный коэффициент для пересчёта удельного объёма на температуру теплоносителя К t"]
[null,null,null,"50оС","60оС","70оС","80оС","90оС","100оС"]
[null,null,null,3.03,2.13,1.59,1.23,1,0.82]
[]
[{"$nulls":6},"Таблица 4: Объём системы отопления, VA=Q*K tS(m*v), л"]
[{"$nulls":4},"Q, кВт","K t","S(m*v), л/кВт",null,"VА, л"]
[{"$nulls":4},0,1,0,null,456]
[]
[{"$nulls":7},"Известный объём системы отопления, л VA=",null,"л"]
[]
[{"$nulls":9},"Объём теплоносителя DIXIS-65 при температуре замерзания - 30оС VD-65=",301,"л"]
[]
[null,null,"Объём расширения теплоносителя, Ve=",{"$nulls":5},"VA*n",", л"]
[{"$nulls":8},100]
[]
[{"$nulls":5},"Ve=",13.20576,",л"]
[]
[{"$nulls":6},"Начальный объём теплоносителя в расширительном баке"]
[]
[{"$nulls":5},"3 л<VV=","VA*0,5",", л"]
[{"$nulls":6},100]
[]
[{"$nulls":5},"V'V=",3,", л"]
[]
[{"$nulls":5},"V\"V=",5.1000000000000005,", л (при Vn<15 л)"]
[]
[{"$nulls":6},"Конечное давление pe=pSV-dPA+hSV, л (до pSV=5 бар, dPA=0,5 бар, при pSV>5 бар, dPA=0,05pSV)"]
[]
[{"$nulls":5},"ре=",2.65,",бар"]
[]
[null,null,"Номинальный объём расширительного бака Vn мин=(Ve+Vv)",{"$nulls":7},"pe+1",", л"]
[{"$nulls":10},"pe+po"]
[]
[{"$nulls":6},"Расчётное давление Рро= Pst+PD, бар. РD= 0 бар до 100оС, =0,5 бар от 100 до110оС и =1бар от 110 до 120оС"]
[{"$nulls":6},"Давление газа в расширительном баке в незаполненной системе отопления:"]
[{"$nulls":5},"Рро=",0.33,",бар"]
[]
[{"$nulls":5},"V'n мин =",25.5,",л"]
[{"$nulls":5},"V\"n мин =",28.810000000000002,",л"]
[]
[{"$nulls":6},"Минимальный номинальный объём расширительного бака"]
[{"$nulls":5},"Vn мин =",26,",л"]
[]
[{"$nulls":6},"Таблица 6(справочная): Номинальные размеры расширительных баков ELBI, л"]
[null,null,8,24,35,50,80,100,150,200,500]
[]
[{"$nulls":6},"Фактический объём расширительного бака (по каталогу)"]
[]
[{"$nulls":5},"Vn(Н)=",10,", л"]
[]
[{"$nulls":6},"Фактический начальный объём жидкости в баке"]
[]
[{"$nulls":5},"VV'=",-6.8999999999999995,", л"]
[]
[{"$nulls":6},"Начальное давление в точке подключения расширительного бака"]
[{"$nulls":6},"в холодной системе"]
[]
[{"$nulls":5},"Pa=",-0.30000000000000004,", бар"]
[]
[]
[]
[]
[]
[]
[null,"Таблицы 7: Состав системы отопления"]
[]
[null,"Трубопроводы "]
[]
[null,"Наименование",{"$nulls":4},"Внутр. диам, мм",null,"Длина, м",null,"Объём, л"]
[null,"Трубы стальные"]
[null,"Труба стальная водогазопроводная Ду15, пог. м",{"$nulls":4},15.7,null,null,null,0]
[null,"Труба стальная водогазопроводная Ду20, пог. м",{"$nulls":4},21.2,null,null,null,0]
[null,"Труба стальная водогазопроводная Ду25, пог. м",{"$nulls":4},27.1,null,null,null,0]
[null,"Труба стальная водогазопроводная Ду32, пог. м",{"$nulls":4},35.9,null,null,null,0]
[null,"Труба стальная водогазопроводная Ду40, пог. м",{"$nulls":4},41,null,null,null,0]
[null,"Труба стальная водогазопроводная Ду50, пог. м",{"$nulls":4},53,null,null,null,0]
[null,"Труба стальная  76х3, пог. м",{"$nulls":4},70,null,null,null,0]
[null,"Труба стальная  89х3,5, пог. м",{"$nulls":4},82,null,null,null,0]
[null,"Труба стальная  108х4, пог. м",{"$nulls":4},100,null,null,null,0]
[null,"Труба стальная  133х4, пог. м",{"$nulls":4},125,null,null,null,0]
[null,"Труба стальная  159х4,5, пог. м",{"$nulls":4},150,null,null,null,0]
[null,"Трубы медные"]
[null,"Труба медная  15х1",{"$nulls":4},13,null,null,null,0]
[null,"Труба медная  18х1",{"$nulls":4},16,null,null,null,0]
[null,"Труба медная  22х1",{"$nulls":4},20,null,null,null,0]
[null,"Труба медная  28х1",{"$nulls":4},26,null,null,null,0]
[null,"Труба медная  35х1,5",{"$nulls":4},32,null,null,null,0]
[null,"Труба медная  42х1,5",{"$nulls":4},39,null,null,null,0]
[null,"Труба медная  54х1",{"$nulls":4},52,null,null,null,0]
[null,"Трубы полипропиленовые PN20"]
[null,"Труба полипропиленовая  16*2,7",{"$nulls":4},10.6,null,null,null,0]
[null,"Труба полипропиленовая  20*3,4",{"$nulls":4},13.2,null,null,null,0]
[null,"Труба полипропиленовая  25*4,2",{"$nulls":4},16.6,null,null,null,0]
[null,"Труба полипропиленовая  32*5,4",{"$nulls":4},21.2,null,null,null,0]
[null,"Труба полипропиленовая  40*6,7",{"$nulls":4},26.6,null,null,null,0]
[null,"Труба полипропиленовая  50*8,4",{"$nulls":4},33.2,null,null,null,0]
[null,"Труба полипропиленовая  63*10,5",{"$nulls":4},42,null,null,null,0]
[null,"Труба полипропиленовая  75*12,5",{"$nulls":4},50,null,null,null,0]
[null,"Труба полипропиленовая  90*15",{"$nulls":4},60,null,null,null,0]
[null,"Трубы металлопластиковые HENKO"]
[null,"Труба металлопластиковая 14х2, пог. м",{"$nulls":4},10,null,null,null,0]
[null,"Труба металлопластиковая 16х2, пог. м",{"$nulls":4},12,null,842.5,null,95.24000000000001]
[null,"Труба металлопластиковая 20х2, пог. м",{"$nulls":4},16,null,1,null,0.21000000000000002]
[null,"Труба металлопластиковая 26х3, пог. м",{"$nulls":4},20,null,1,null,0.32]
[null,"Труба металлопластиковая 32х3, пог. м",{"$nulls":4},26,null,72,null,38.21]
[{"$nulls":6},"Общий объём воды в трубах, л",null,null,null,134]
[{"$nulls":12},916.5]
[{"$nulls":4},"Радиаторы алюминиевые ТОР"]
[]
[{"$nulls":4},"Тип радиатора",null,"Колич. секций",null,"Кол., шт","Объём воды, л"]
[{"$nulls":4},"ТОР-R 35",null,1,null,null,0]
[{"$nulls":6},2,null,null,0]
[{"$nulls":6},3,null,null,0]
[{"$nulls":6},4,null,null,0]
[{"$nulls":6},5,null,null,0]
[{"$nulls":6},6,null,null,0]
[{"$nulls":6},7,null,null,0]
[{"$nulls":6},8,null,null,0]
[{"$nulls":6},9,null,null,0]
[{"$nulls":6},10,null,null,0]
[{"$nulls":6},11,null,null,0]
[{"$nulls":6},12,null,null,0]
[{"$nulls":6},13,null,null,0]
[{"$nulls":6},14,null,null,0]
[{"$nulls":6},15,null,null,0]
[{"$nulls":6},16,null,null,0]
[{"$nulls":6},17,null,null,0]
[{"$nulls":6},18,null,null,0]
[{"$nulls":6},19,null,null,0]
[{"$nulls":6},20,null,null,0]
[{"$nulls":4},"ТОР-R 50",null,1,null,null,0]
[{"$nulls":6},2,null,null,0]
[{"$nulls":6},3,null,null,0]
[{"$nulls":6},4,null,null,0]
[{"$nulls":6},5,null,null,0]
[{"$nulls":6},6,null,null,0]
[{"$nulls":6},7,null,null,0]
[{"$nulls":6},8,null,null,0]
[{"$nulls":6},9,null,null,0]
[{"$nulls":6},10,null,null,0]
[{"$nulls":6},11,null,null,0]
[{"$nulls":6},12,null,null,0]
[{"$nulls":6},13,null,null,0]
[{"$nulls":6},14,null,null,0]
[{"$nulls":6},15,null,null,0]
[{"$nulls":6},16,null,null,0]
[{"$nulls":6},17,null,null,0]
[{"$nulls":6},18,null,null,0]
[{"$nulls":6},19,null,null,0]
[{"$nulls":6},20,null,null,0]
[{"$nulls":4},"Общий объём воды в радиаторах ТОР, л",{"$nulls":4},0]
[]
[]
[{"$nulls":4},"Радиаторы алюминиевые Super TWIST"]
[]
[{"$nulls":4},"Тип радиатора",null,"Колич. секций",null,"Кол., шт","Объём воды, л"]
[{"$nulls":4},"Super TWIST 35",null,1,null,null,0]
[{"$nulls":6},2,null,null,0]
[{"$nulls":6},3,null,null,0]
[{"$nulls":6},4,null,null,0]
[{"$nulls":6},5,null,null,0]
[{"$nulls":6},6,null,null,0]
[{"$nulls":6},7,null,null,0]
[{"$nulls":6},8,null,null,0]
[{"$nulls":6},9,null,null,0]
[{"$nulls":6},10,null,null,0]
[{"$nulls":6},11,null,null,0]
[{"$nulls":6},12,null,null,0]
[{"$nulls":6},13,null,null,0]
[{"$nulls":6},14,null,null,0]
[{"$nulls":6},15,null,null,0]
[{"$nulls":6},16,null,null,0]
[{"$nulls":6},17,null,null,0]
[{"$nulls":6},18,null,null,0]
[{"$nulls":6},19,null,null,0]
[{"$nulls":6},20,null,null,0]
[{"$nulls":4},"Super TWIST 50",null,1,null,null,0]
[{"$nulls":6},2,null,null,0]
[{"$nulls":6},3,null,null,0]
[{"$nulls":6},4,null,null,0]
[{"$nulls":6},5,null,null,0]
[{"$nulls":6},6,null,null,0]
[{"$nulls":6},7,null,null,0]
[{"$nulls":6},8,null,null,0]
[{"$nulls":6},9,null,null,0]
[{"$nulls":6},10,null,null,0]
[{"$nulls":6},11,null,null,0]
[{"$nulls":6},12,null,null,0]
[{"$nulls":6},13,null,null,0]
[{"$nulls":6},14,null,null,0]
[{"$nulls":6},15,null,null,0]
[{"$nulls":6},16,null,null,0]
[{"$nulls":6},17,null,null,0]
[{"$nulls":6},18,null,null,0]
[{"$nulls":6},19,null,null,0]
[{"$nulls":6},20,null,null,0]
[{"$nulls":4},"Общий объём воды в радиаторах ТОР, л",{"$nulls":4},0]
[]
[]
[{"$nulls":4},"Радиаторы алюминиевые CF"]
[]
[{"$nulls":4},"Тип радиатора",null,"Колич. секций",null,"Кол., шт","Объём воды, л"]
[{"$nulls":4},"CF-300",null,1,null,null,0]
[{"$nulls":6},2,null,null,0]
[{"$nulls":6},3,null,null,0]
[{"$nulls":6},4,null,null,0]
[{"$nulls":6},5,null,null,0]
[{"$nulls":6},6,null,null,0]
[{"$nulls":6},7,null,null,0]
[{"$nulls":6},8,null,null,0]
[{"$nulls":6},9,null,null,0]
[{"$nulls":6},10,null,null,0]
[{"$nulls":6},11,null,null,0]
[{"$nulls":6},12,null,null,0]
[{"$nulls":6},13,null,null,0]
[{"$nulls":6},14,null,null,0]
[{"$nulls":6},15,null,null,0]
[{"$nulls":6},16,null,null,0]
[{"$nulls":6},17,null,null,0]
[{"$nulls":6},18,null,null,0]
[{"$nulls":6},19,null,null,0]
[{"$nulls":6},20,null,null,0]
[{"$nulls":4},"CF-500",null,1,null,null,0]
[{"$nulls":6},2,null,null,0]
[{"$nulls":6},3,null,null,0]
[{"$nulls":6},4,null,null,0]
[{"$nulls":6},5,null,null,0]
[{"$nulls":6},6,null,null,0]
[{"$nulls":6},7,null,null,0]
[{"$nulls":6},8,null,null,0]
[{"$nulls":6},9,null,null,0]
[{"$nulls":6},10,null,null,0]
[{"$nulls":6},11,null,null,0]
[{"$nulls":6},12,null,null,0]
[{"$nulls":6},13,null,null,0]
[{"$nulls":6},14,null,null,0]
[{"$nulls":6},15,null,null,0]
[{"$nulls":6},16,null,null,0]
[{"$nulls":6},17,null,null,0]
[{"$nulls":6},18,null,null,0]
[{"$nulls":6},19,null,null,0]
[{"$nulls":6},20,null,null,0]
[{"$nulls":4},"CF-600",null,1,null,null,0]
[{"$nulls":6},2,null,null,0]
[{"$nulls":6},3,null,null,0]
[{"$nulls":6},4,null,null,0]
[{"$nulls":6},5,null,null,0]
[{"$nulls":6},6,null,null,0]
[{"$nulls":6},7,null,null,0]
[{"$nulls":6},8,null,null,0]
[{"$nulls":6},9,null,null,0]
[{"$nulls":6},10,null,null,0]
[{"$nulls":6},11,null,null,0]
[{"$nulls":6},12,null,null,0]
[{"$nulls":6},13,null,null,0]
[{"$nulls":6},14,null,null,0]
[{"$nulls":6},15,null,null,0]
[{"$nulls":6},16,null,null,0]
[{"$nulls":6},17,null,null,0]
[{"$nulls":6},18,null,null,0]
[{"$nulls":6},19,null,null,0]
[{"$nulls":6},20,null,null,0]
[{"$nulls":4},"Общий объём воды в радиаторах ТОР, л",{"$nulls":4},0]
[]
[]
[{"$nulls":4},"Радиаторы стальные  (HENRAD)"]
[]
[{"$nulls":4},"Тип радиатора",null,"Высота","Длина","Кол., шт","Объём воды, л"]
[{"$nulls":4},"11К(V)",null,300,600,null,0]
[{"$nulls":7},800,null,0]
[{"$nulls":7},900,null,0]
[{"$nulls":7},1000,null,0]
[{"$nulls":7},1200,null,0]
[{"$nulls":7},1400,null,0]
[{"$nulls":7},1600,null,0]
[{"$nulls":7},1800,null,0]
[{"$nulls":7},2000,null,0]
[{"$nulls":7},2200,null,0]
[{"$nulls":7},2400,null,0]
[{"$nulls":7},2600,null,0]
[{"$nulls":7},2800,null,0]
[{"$nulls":7},3000,null,0]
[{"$nulls":6},500,400,null,0]
[{"$nulls":7},500,2,2.8]
[{"$nulls":7},600,null,0]
[{"$nulls":7},700,null,0]
[{"$nulls":7},800,1,2.24]
[{"$nulls":7},900,null,0]
[{"$nulls":7},1000,null,0]
[{"$nulls":7},1100,null,0]
[{"$nulls":7},1200,null,0]
[{"$nulls":7},1400,null,0]
[{"$nulls":7},1600,null,0]
[{"$nulls":7},1800,null,0]
[{"$nulls":7},2000,null,0]
[{"$nulls":7},2200,null,0]
[{"$nulls":7},2400,null,0]
[{"$nulls":7},2600,null,0]
[{"$nulls":7},2800,null,0]
[{"$nulls":7},3000,null,0]
[{"$nulls":4},"22К(V)",null,300,600,null,0]
[{"$nulls":7},800,null,0]
[{"$nulls":7},900,null,0]
[{"$nulls":7},1000,null,0]
[{"$nulls":7},1200,null,0]
[{"$nulls":7},1400,null,0]
[{"$nulls":7},1600,null,0]
[{"$nulls":7},1800,null,0]
[{"$nulls":7},2000,null,0]
[{"$nulls":7},2200,null,0]
[{"$nulls":7},2400,null,0]
[{"$nulls":7},2600,null,0]
[{"$nulls":7},2800,null,0]
[{"$nulls":7},3000,null,0]
[{"$nulls":6},500,400,null,0]
[{"$nulls":7},500,1,2.82]
[{"$nulls":7},600,4,13.52]
[{"$nulls":7},700,1,3.9499999999999997]
[{"$nulls":7},800,5,22.52]
[{"$nulls":7},900,8,40.54]
[{"$nulls":7},1000,1,5.63]
[{"$nulls":7},1100,null,0]
[{"$nulls":7},1200,3,20.270000000000003]
[{"$nulls":7},1400,1,7.89]
[{"$nulls":7},1600,null,0]
[{"$nulls":7},1800,1,10.14]
[{"$nulls":7},2000,null,0]
[{"$nulls":7},2200,2,24.78]
[{"$nulls":7},2400,null,0]
[{"$nulls":7},2600,null,0]
[{"$nulls":7},2800,null,0]
[{"$nulls":7},3000,null,0]
[{"$nulls":4},"33К(V)",null,300,600,null,0]
[{"$nulls":7},800,null,0]
[{"$nulls":7},900,null,0]
[{"$nulls":7},1000,null,0]
[{"$nulls":7},1200,null,0]
[{"$nulls":7},1400,null,0]
[{"$nulls":7},1600,null,0]
[{"$nulls":7},1800,null,0]
[{"$nulls":7},2000,null,0]
[{"$nulls":7},2200,null,0]
[{"$nulls":7},2400,null,0]
[{"$nulls":7},2600,null,0]
[{"$nulls":7},2800,null,0]
[{"$nulls":7},3000,null,0]
[{"$nulls":6},500,400,null,0]
[{"$nulls":7},500,null,0]
[{"$nulls":7},600,null,0]
[{"$nulls":7},700,null,0]
[{"$nulls":7},800,null,0]
[{"$nulls":7},900,null,0]
[{"$nulls":7},1000,null,0]
[{"$nulls":7},1100,null,0]
[{"$nulls":7},1200,null,0]
[{"$nulls":7},1400,null,0]
[{"$nulls":7},1600,null,0]
[{"$nulls":7},1800,null,0]
[{"$nulls":7},2000,null,0]
[{"$nulls":7},2200,null,0]
[{"$nulls":7},2400,null,0]
[{"$nulls":7},2600,null,0]
[{"$nulls":7},2800,null,0]
[{"$nulls":7},3000,null,0]
[{"$nulls":4},"Общий объём воды в радиат. W. Line, л",{"$nulls":4},158]
[]
[]
[{"$nulls":7},"Объём теплоносителя в отопительном котлах"]
[{"$nulls":4},"Марка котла",null,"Объём,V","Число котлов",null,"Объём общий"]
[{"$nulls":4},"Alfa G,GP",null,56,null,null,0]
[{"$nulls":4},"Alfa Sprint S,SV,M,MV",null,60,null,null,0]
[{"$nulls":4},"Alfa F,FV",null,60,null,null,0]
[{"$nulls":4},"Delta Classic G20",null,114.5,null,null,0]
[{"$nulls":4},"Delta Classic G25,G30,P30",null,87.5,null,null,0]
[{"$nulls":4},"Delta Performance ,-G,-F 25",null,83,null,null,0]
[{"$nulls":4},"Delta Performance ,-G,-F 35",null,104,null,null,0]
[{"$nulls":4},"Delta Performance ,-G,-F 45",null,70,null,null,0]
[{"$nulls":4},"Delta Performance ,-G,-F 55",null,82,null,null,0]
[{"$nulls":4},"Delta F25 HR",null,83,null,null,0]
[{"$nulls":4},"Delta F35 HR",null,114.5,null,null,0]
[{"$nulls":4},"Delta F45 HR",null,62.5,null,null,0]
[{"$nulls":4},"Heat Master HM 60 N",null,82,null,null,0]
[{"$nulls":4},"Heat Master HM 70 N, 71",null,108,null,null,0]
[{"$nulls":4},"Heat Master HM 100 N, 101",null,130,null,null,0]
[{"$nulls":4},"Heat Master HM Jumbo",null,245,null,null,0]
[{"$nulls":4},"GN 52",null,57,null,null,0]
[{"$nulls":4},"GN 62",null,66,null,null,0]
[{"$nulls":4},"GN 72",null,74,null,null,0]
[{"$nulls":4},"GN 82",null,90,null,null,0]
[{"$nulls":4},"N 0",null,31,null,null,0]
[{"$nulls":4},"N 1",null,31,null,null,0]
[{"$nulls":4},"N2",null,37,null,null,0]
[{"$nulls":4},"N 3",null,53,null,null,0]
[{"$nulls":4},"CA 100",null,102,null,null,0]
[{"$nulls":4},"CA 150",null,122,1,null,122]
[{"$nulls":4},"CA 200",null,150,null,null,0]
[{"$nulls":4},"CA 250",null,350,null,null,0]
[{"$nulls":4},"CA 300",null,400,null,null,0]
[{"$nulls":4},"CA 350",null,470,null,null,0]
[{"$nulls":4},"CA 400",null,630,null,null,0]
[{"$nulls":4},"CA 500",null,650,null,null,0]
[{"$nulls":4},"CA 600",null,800,null,null,0]
[{"$nulls":4},"CA 700",null,890,null,null,0]
[{"$nulls":4},"CA 800",null,920,null,null,0]
[{"$nulls":4},"CA 900",null,1030,null,null,0]
[{"$nulls":4},"CA 1000",null,1140,null,null,0]
[{"$nulls":4},"ET-,ETS 09",null,13,null,null,0]
[{"$nulls":4},"ET-,ETS 15",null,13,null,null,0]
[{"$nulls":4},"ET-,ETS 24",null,13,null,null,0]
[{"$nulls":4},"TER 28,8 -- 144",null,155,null,null,0]
[{"$nulls":4},"TER 201 и -259",null,250,null,null,0]
[{"$nulls":4},"РусНИТ 203-204",null,5,null,null,0]
[{"$nulls":4},"РусНИТ 205-209",null,7,null,null,0]
[{"$nulls":4},"РусНИТ 212-224",null,12,null,null,0]
[{"$nulls":4},"РусНИТ 230-245",null,18,null,null,0]
[{"$nulls":4},"РусНИТ 270-2100",null,26,null,null,0]
[{"$nulls":4},"АОГВ-11",null,33,null,null,0]
[{"$nulls":4},"АОГВ-17",null,63,null,null,0]
[{"$nulls":4},"АОГВ-23",null,62,null,null,0]
[{"$nulls":4},"АОГВ-29",null,64,null,null,0]
[{"$nulls":4},"АКГВ-23",null,60,null,null,0]
[{"$nulls":4},"АКГВ-29",null,58,null,null,0]
[{"$nulls":4},"Wester Ecо WE 3",null,8.2,null,null,0]
[{"$nulls":4},"Wester Ecо WE 4",null,10,null,null,0]
[{"$nulls":4},"Wester Ecо WE 5",null,11.8,null,null,0]
[{"$nulls":4},"Wester Ecо WE 6",null,13.6,null,null,0]
[{"$nulls":4},"Wester Ecо WE 7",null,15.4,null,null,0]
[{"$nulls":9},0]
[{"$nulls":4},"Общий объём теплоносителя в котлах, л",{"$nulls":4},122]
[]
[{"$nulls":7},"Объём теплоносителя в бойлерах"]
[null,null,null,"Марка бойлера",null,null,"Объём отоп. конт.",null,"Число бойлеров",null,"Объём общий"]
[null,null,null,"HL E 100",null,null,30,null,null,null,0]
[null,null,null,"HL E 130",null,null,31,null,null,null,0]
[null,null,null,"HL E 160",null,null,35,null,null,null,0]
[null,null,null,"HL E 210",null,null,39,null,null,null,0]
[null,null,null,"HL E 240",null,null,42,null,1,null,42]
[null,null,null,"Smart Line SL 100",null,null,30,null,null,null,0]
[null,null,null,"Smart Line SL 130",null,null,31,null,null,null,0]
[null,null,null,"Smart Line SL 160",null,null,35,null,null,null,0]
[null,null,null,"Smart Line SL 210",null,null,39,null,null,null,0]
[null,null,null,"Smart Line SL 240",null,null,42,null,null,null,0]
[null,null,null,"Smart Line SL 320",null,null,55,null,null,null,0]
[null,null,null,"HR Duplex 321",null,null,55,null,null,null,0]
[null,null,null,"HR Duplex 601",null,null,161,null,null,null,0]
[null,null,null,"Jumbo 800",null,null,125,null,null,null,0]
[null,null,null,"Jumbo 1000",null,null,160,null,null,null,0]
[null,null,null,"Общий объём теплоносителя в бойлерах, л",{"$nulls":6},42]
[]
[]
[null,null,null,"Общий объём теплоносителя в системе, л",{"$nulls":6},456]