{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":21,"n_cols":12,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Тип","Описание","Производитель","Модель",null,"Состояние","Кол-во","Цена нового","Цена","Примечание"]
[null,"Контроллер","Модуль 10DI , Lon","Schneider","Xenta 411 v1.05",7302011,"нов",1,20000,10000]
[null,"Контроллер","Контроллер ,  4DI 6DO 4UI 4TI 2AO, Lon","Schneider","Xenta 301 v3.87",7300132,"нов",1,50000,25000]
[null,"Датчик","Датчик температуры погружной STP100-50. 1.8кОм.50мм","Schneider","STP100-50 ",5123102010,"нов",2,5300,2000]
[null,"Датчик","Гильза из нержавеющей стали PN25","Schneider","Schneider",9121050000,"нов",3,5300,2000]
[null,"Датчик","Датчик температуры погружной, LG-Ni1000, 100 мм, -30...130 C, IP42","Siemens","QAE2120,010",null,"БУ",1,null,300]
[null,"Датчик","Датчик комнатный NTC10k +/-1%","epluse"," ee10-m7tp14vn0",null,"нов",1,null,1000,null,"https://epluse-group.ru/fileadmin/data/product/ee10_t/datasheet_EE10-T.pdf"]
[null,"Датчик","Датчик температуры погружной, Pt1000, 100 мм, -30...130 C, IP42","Siemens","QAE2112.010",null,"нов",1,2000,1000,"2 тыс -10 тыс ?"]
[null,"Датчик","датчик наружной температуры, PT1000","Siemens","QAC2012",null,"нов ?",1,1400,1000]
[null,"Датчик","датчик наружной температуры, NTC 575","Siemens","QAC31/101",null,"нов ?",1,1100,500]
[null,"Датчик","Датчик температуры канальный, 40 см, LG-Ni 1000, -50..+80","Siemens","QAM2120.040",null,"БУ",1,null,300]
[null,"Датчик","Датчики -50..180, с разъемом","?","ТМ04-50М.В3.35/3.15",null,"нов ?",3,null,500,"Для контроля температуры двигателей?3 комплекта, в каждом по 3 шт."]
[null,"Для щита","Контактор модульный 4Kw, 3P + 1NO , 9A , катушка 24VAC/VDC","ABB","ESB25-40N-01","1SAE231111R0140","нов",1,5100,2500]
[null,"Для щита","Контактор 2,2kW, 3P + 1NO , 6A , катушка 230VAC","Schneider","LC1K0610M7",null,"нов",2,4500,2500]
[null,"Прочее","Ethernet MODBUS Metering Interface Controller","Trend","EMIC/MDA/16",null,"БУ",1,null,"догов.","используется только с контроллерами и BMS от Trend","https://partners.trendcontrols.com/trendproducts/cd/ru/pdf/en-ta201081-uk0yr0715h.pdf"]
[null,"Прочее","Счетчик импульсов 2-хканальный, RS485, питание 7..25 VDC","Пульсар (НПП Тепловодохран)","Пульсар",null,"БУ",2,2700,1000,"1 использовался при наладке","https://pulsarm.ru/upload/iblock/7ae/7ae49f0cf8eb3a61f5978806a1f15996.pdf"]
[null,"Прочее","Преобразователь CAN в Ethernet","ICP-DAS","I7540-G CR ","I7540DCR01LHAFI00010","БУ",1,20000,10000,"новый 330$ \nиспользовался при наладке","https://icpdas.ru/catalogue/converters_gateways/converters/can_converter/i-7540d-g-cr/"]
[null,"Прочее","Ручной программатор HPG-3 (для программирования и снятия показаний компактных M-Bus и дополнительных модулей M-Bus счетчиков воды ЕТ и Истаметр М","Ista","Ista HPG-3 v4.0",null,"БУ",1,12000,6000,"использовался при наладке"]
[null,"Прочее","Беспроводная двухдиапазонная точка доступа / мост N450","D-Link","DAP-1533",null,"БУ",1,null,1000,"использовался при наладке","https://dlink.ru/ru/products/2/1609.html"]
[null,null,"Патч-корд UTP",null,null,null,"нов",5,200,100,"100-600"]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}