{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":16,"n_cols":11,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[null,null,"R, м2*С/Вт"]
[null,"Наружные стены",null,null,"Пол 1зона",2.13]
[null,"Окна",null,null,"Пол 2зона",4.29]
[null,"Кровля",null,null,"Пол 3зона",8.62]
[null,"Пол в подвале",null,null,"Пол 4зона",14.28]
[null,"Перекрытие (Пр)"]
[null,"Внутренняя стена"]
["   № помещ.","Наименование","Огр.конструкц.","Ориентация","Площадь, кв.м","R, кв.м*С/Вт","tв, С","tн, С","tв-tн, С","добавка","Q=S*t*m/R,Вт"]
[null,"План на отм. 0.000; -0.450"]
[null,"Пол 1з",null,null,1184,2.13,18,-31,49,1,27237.558685446013]
[null,"Пол 2з",null,null,1152,4.29,18,-31,49,1,13158.041958041958]
[null,"Пол 3з",null,null,1120,8.62,18,-31,49,1,6366.589327146172]
[null,"Пол 4з",null,null,19044,14.28,18,-31,49,1,65347.05882352941]
[]
[{"$nulls":9},"Сумма",112109.24879416355]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}