{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":20,"n_cols":16,"rows_kept":20,"cut":false,"hidden":false,"merged":[[9,5,10,10],[4,5,5,11],[16,5,17,9],[9,12,10,15]],"flags":["formulas_cached_only"]}
[]
[]
[null,null,"Температуа теплоносителля"]
[null,"Т1",80]
[null,"Т2",60,null,null,"Ekoplastik Stabi PN20"]
[]
[null,null,"Тепловая нагрузка, Вт",null,"Диаметр (наружный)",20,25,32,40,50,63,75]
[null,null,25000,null,"Скорость, м/с",1.8341428475685224,1.1738514224438543,0.7066138913343654,0.4522328904539938,0.29022912981274135,0.18131226562794803,0.12851692963066635]
[null,null,"Расход воды, кг/ч"]
[null,null,1074.8065348237317,null,null,"ГОСТ 3262 (обыкновенные)",{"$nulls":6},"ГОСТ 10704-91"]
[]
[{"$nulls":4},"Диаметр (условный)",15,20,25,32,40,50,null,"76х3","89х3","108х4","133х4"]
[{"$nulls":4},"Скорость, м/с",1.542974809817067,0.8462261055353525,0.5178685759613959,0.295100023177822,0.2262509582818613,0.1353961768856564,null,0.07761793079016506,0.0552079925782855,0.03803278608718088,0.024340983095795764]
[{"$nulls":4},"диаметр наруж.",21.3,26.8,33.5,42.3,48,60]
[]
[]
[{"$nulls":5},"Kisan (металлопластиковые)"]
[]
[{"$nulls":4},"Диаметр (наружный)",16,20,25,32,40]
[{"$nulls":4},"Скорость, м/с",2.6411657004986724,1.58305040945602,0.9508196521795219,0.5626151788044509,0.3714139266326258]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}